# ¶ Zappi EV charger

We are using this homeassistant custom integration to connect to the myenergi system, which also gives us control to the Eddi solar diverter.

## ¶ Add Myenergi integration

- Go to Settings -> Devices & Services

- You should now be on the integrations page, choose "Add integration"

- You can either find myenergi in the list or type the first few letters to auto-sort.

- Double clicking the integration starts the install process, after two minutes you will be asked for user credentials

## ¶ Entering User credentials

- Enter the serial number of the device (which is printed on the device itself), this could be the zappi for newer internet connected models or the myenergi hub.
- The second box requires the customers myenergi password or an API key for https://myaccount.myenergi.com
  We recommend asking the user to create an API key* on their myenergi account as it means we don't have access to the user password and the the user retains the right to withdraw access.

## ¶ Setting up the local energy dashboard

- Selection 'Energy' in the left side bar to setup your local energy dashboard. Below are the fields which should be entered in each location.

- You dashboard should now appear as follows